컴퓨터를 이용한 치아크기 계측시 재현도와 정확도에 관한 연구

김 은 정

전남대학교 대학원 치의학과

(지도교수 : 박병주)

(초록)

본 연구는 치아크기 측정시 버니어 캘리퍼스를 사용한 계측치와 석고모형을 촬영하여 컴퓨터를 사용한 계측치를 서로 비교함으로써 석고모형 분석시 컴퓨터 이용 가능성을 알아보고자 시행되었다. 치아밀집 치열 특징을 지니며 모든 치아의 맹출이 완료된 상하악 20조의 석고모형의 좌측 중절치부터 제1대구치까지 12개의 치아를 대상으로 하여, 각 치아의 근원심폭경을 버니어 캘리퍼스와 컴퓨터를 이용하여 2주 간격으로 2회 측정하여 실험 측정치를 얻은 다음, 측정에 이용된 석고모형을 근원심 접촉점 부위에서 개개치아로 분리한 후, 마이크로미터를 이용하여 측정한 표준치와 비교분석하였다. 계측치 오차의 원인을 알아보기 위하여 상하악의 occlusogram을 얻어 각 치아의 접촉점 이탈유무 및 정도를 구하고, TARG를 이용하여 각 치아의 근원심 경사도를 계측한 결과 다음과 같은 결론을 얻었다.

1. 2회 측정에 대한 재현도 비교시 버니어 캘리퍼스를 사용한 경우 12개 치아중 3개의 치아에서 유의한 차이가 나타났으며 컴퓨터의 경우에는 1개의 치아에서 차이가 나타났다.

2. 치아크기 계측의 정확도를 알아보기 위하여 표준치와 비교한 결과, 버니어 캘리퍼스를 사용한 경우 12개 중 3개의 치아에서 유의한 차이가 있었으며 컴퓨터의 경우에는 12개 중 2개의 치아에서 차이가 나타났다.

3. 버니어 켈리퍼스를 사용한 경우 상악 제1대구치는 표준치에 비해 크게, 하악 제1대구치는 표준치에 비해 작게 재는 경향을 보였으며 컴퓨터의 경우 상하 제1대구치 모두 표준치에 비해 크게 재는 경향을 보였다.

4. 버니어 캘리퍼스로 계측시에는 하악 제1대구치가 가장 큰 오차를 보였으며 치아별로 오차 정도가 다양하게 나타난 반면, 컴퓨터의 경우 치아별 오차정도의 차이를 보이지 않았다.

5. 접촉점 이탈정도 및 치관의 근원심 경사도와 오차정도의 상관관계를 살펴본 결과 버니어 켈리퍼스로 측정한 경우 유의한 상관관계를 보이지 않았으나 컴퓨터로 계측한 경우 약한 순상관관계를 보였다.

이상의 결과는 모형분석을 위한 치아크기 계측시 컴퓨터 이용이 가능함을 시사하였다.

Reproducibility and Accuracy of Tooth Size Measurements Obtained by the Use of Computer

Eun-Jeong Kim

Faculty of Dentistry

Graduate School, Chonnam National University, Kwangju, Korea

(Directed by Associate Professor Byung-Ju Park)

(Abstract)

The purpose of this study is to evaluate the availability of computer system for the measurement of tooth size in the model analysis through the comparison of two measurements: One is to use a computer; and the other is to use vernier calipers. 20 sets of casts were used, which showed a moderate degree of crowding and full eruption of all teeth. The mesio-distal width of 12 teeth from the left central incisor to the left first molar at each set of the casts were measured twice with vernier calipers and a computer respectively. This measurement was repeated two weeks later. First, for the reproducibility analysis, the two computer measurements were compared then the vernier calipers measurements were compared. Second, all the teeth were sepapated into the region of mesiodistal contact points and its width was measured by a micrometer to obtain standard measurements. For the accuracy analysis, these standard measurements were compared with the measurements from the dental casts using two methods. The difference between them was defined as the measurement error in due course. To investigate the cause of measurement error, an examination was made for the presence and degree of contact point deviation on each tooth in terms of upper and lower occlusogram, and the mesio-distal angulation of each tooth was measured with TARG.

The following are the results of the analysis:

1. In the analysis for reproducibility; the measurements with vernier calipers showed       significant differences in three out of twelve teeth while the computer measurements     showed significant differences in one out of twelve teeth.

2. In the analysis for accuracy; compared with the standard measurements, the            measurements with vernier calipers showed significant differences in three out of        twelve teeth while the computer measurements showed significant differences in two     out of twelve teeth.

3. Compared with the standard measurements, the measurements with vernier calipers were apt to be larger at the upper first molar, and smaller at the lower first molar. The computer measurements, however, were apt to be larger at both lower and upper first molars.

4. The measurements with vernier calipers showed the largest error at the lower first molar and the degree of error was variable according to the tooth while the difference of error was minimal in the computer measurements.

5. In the analysis for the correlation of the degree of measurement errors with the contact point deviation index and the mesio-distal crown angulation of each tooth, the measurements with vernier calipers did not show significant correlation while the measurements with computer showed slight positive correlations.

The results of this study indicate that a computer system may be useful for the measurement of tooth size in the model analysis.